1. “Optimizing Er/Yb ratio and content in Er-Yb co-doped glass-ceramics for enhancement of the up- and down-conversion luminescence”. Tikhomirov VK, Rodríguez VD, Méndez-Ramos J, del- Castillo J, Kirilenko D, Van Tendeloo G, Moshchalkov VV, Solar energy materials and solar cells 100, 209 (2012).   http://doi.org/10.1016/j.solmat.2012.01.019