1. “Preparing polymer films doped with magnetic nanoparticles by spin-coating and melt-processing can induce an in-plane magnetic anisotropy”. Wouters J, Lebedev OI, Van Tendeloo G, Yamada H, Sato N, Vanacken J, Moshchalkov VV, Verbiest T, Valev VK, Journal of applied physics 109, 076105 (2011).   http://doi.org/10.1063/1.3572048