1. “Reliable pore-size measurements based on a procedure specifically designed for electron tomography measurements of nanoporous samples”. Van Eyndhoven G, Batenburg KJ, van Oers C, Kurttepeli M, Bals S, Cool P, Sijbers J,  (2014)