1. “Superior reliability of junctionless pFinFETs by reduced oxide electric field”. Toledano-Luque M, Matagne P, Sibaja-Hernandez A, Chiarella T, Ragnarsson L-A, Sorée B, Cho M, Mocuta A, Thean A, IEEE electron device letters 35, 1179 (2014).   http://doi.org/10.1109/LED.2014.2361769