1. “Multiscale investigation of quasi-brittle fracture characteristics in a 9Cr–1Mo ferritic–martensitic steel embrittled by liquid lead–bismuth under low cycle fatigue”. Gong X, Marmy P, Volodin A, Amin-Ahmadi B, Qin L, Schryvers D, Gavrilov S, Stergar E, Verlinden B, Wevers M, Seefeldt M, Corrosion science 102, 137 (2016).   http://doi.org/10.1016/j.corsci.2015.10.003