1. “Intrinsic tailing of resistive states distributions in amorphous <tex>HfOx </tex> and TaOx based resistive random access memories”. Clima S, Chen YY, Fantini A, Goux L, Degraeve R, Govoreanu B, Pourtois G, Jurczak M, IEEE electron device letters 36, 769 (2015).   http://doi.org/10.1109/LED.2015.2448731