1. “Routes to increase the conversion and the energy efficiency in the splitting of CO2by a dielectric barrier discharge”. Ozkan A, Bogaerts A, Reniers F, Journal of physics: D: applied physics 50, 084004 (2017).   http://doi.org/10.1088/1361-6463/aa562c