1. “Large CO2 uptake on a monolayer of CaO”. Berdiyorov GR, Neek-Amal M, Hussein IA, Madjet ME, Peeters FM, Journal of materials chemistry A : materials for energy and sustainability 5, 2110 (2017).   http://doi.org/10.1039/C6TA08810D