1. “Thermodynamic properties and transport coefficients of a two-temperature polytetrafluoroethylene vapor plasma for ablation-controlled discharge applications”. Wang H, Wang W, Yan JD, Qi H, Geng J, Wu Y, Journal of physics: D: applied physics 50, 395204 (2017).   http://doi.org/10.1088/1361-6463/AA7D68