1. “Carbon dioxide dissociation in a microwave plasma reactor operating in a wide pressure range and different gas inlet configurations”. Belov I, Vermeiren V, Paulussen S, Bogaerts A, Journal of CO2 utilization 24, 386 (2018).   http://doi.org/10.1016/j.jcou.2017.12.009