1. “Controlling the interfacial conductance in LaAlO3/SrTiO3 in 90 degrees off-axis sputter deposition”. Yin C, Krishnan D, Gauquelin N, Verbeeck J, Aarts J, Physical review materials 3, 034002 (2019).   http://doi.org/10.1103/PHYSREVMATERIALS.3.034002