1. “Enzymatic sensor for phenols based on titanium dioxide generating surface confined ROS after treatment with H2O2”. Rahemi V, Trashin S, Hafideddine Z, Meynen V, Van Doorslaer S, De Wael K, Sensors and actuators : B : chemical 283, 343 (2019).   http://doi.org/10.1016/J.SNB.2018.12.039