1. “Macro X-ray fluorescence (MA-XRF) scanning : a new and efficient method for documenting stained-glass panels”. Caen J, Legrand S, van der Snickt G, Janssens K,  (2015)