1. “The use of lead-glass capillaries for microfocusing of highly energetic (0-60 KeV) synchrotron radiation”. Janssens K, Vincze L, Vekemans B, Adams F, Haller M, Knöchel A, Journal of analytical atomic spectrometry 13, 339 (1998).   http://doi.org/10.1039/A707700I