1. “Modeling of the performance of BSCF capillary membranes in four-end and three-end integration mode”. Buysse C, Michielsen B, Middelkoop V, Snijkers F, Buekenhondt A, Kretzschmar J, Lenaerts S, Ceramics international 39, 4113 (2013).   http://doi.org/10.1016/J.CERAMINT.2012.10.266