1. “Bio-electrochemical COD removal for energy-efficient, maximum and robust nitrogen recovery from urine through membrane aerated nitrification”. De Paepe J, De Paepe K, Gòdia F, Rabaey K, Vlaeminck SE, Clauwaert P, Water Research 185, 116223 (2020).   http://doi.org/10.1016/J.WATRES.2020.116223