1. “Comparison of four mobile, non‐invasive diagnostic techniques for differentiating glass types in historical leaded windows : MA‐XRF , UV–Vis–NIR, Raman spectroscopy and IRT”. Cagno S, van der Snickt G, Legrand S, Caen J, Patin M, Meulebroeck W, Dirkx Y, Hillen M, Steenackers G, Rousaki A, Vandenabeele P, Janssens K, X-Ray Spectrometry , xrs.3185 (2020).   http://doi.org/10.1002/XRS.3185