1. “Compatibility of Zr₂AlC MAX phase-based ceramics with oxygen-poor, static liquid lead-bismuth eutectic”. Tunca B, Lapauw T, Callaert C, Hadermann J, Delville R, Caspi E'ad N, Dahlqvist M, Rosen J, Marshal A, Pradeep KG, Schneider JM, Vleugels J, Lambrinou K, Corrosion Science 171, 108704 (2020).   http://doi.org/10.1016/J.CORSCI.2020.108704