1. “Early stages of dissolution corrosion in 316L and DIN 1.4970 austenitic stainless steels with and without anticorrosion coatings in static liquid lead-bismuth eutectic (LBE) at 500 degrees C”. Charalampopoulou E, Lambrinou K, Van der Donck T, Paladino B, Di Fonzo F, Azina C, Eklund P, Mraz S, Schneider JM, Schryvers D, Delville R, Materials Characterization 178, 111234 (2021).   http://doi.org/10.1016/J.MATCHAR.2021.111234