1. “Enhancing bioflocculation in high-rate activated sludge improves effluent quality yet increases sensitivity to surface overflow rate”. Van Winckel T, Ngo N, Sturm B, Al-Omari A, Wett B, Bott C, Vlaeminck SE, De Clippeleir H, Chemosphere 308, 136294 (2022).   http://doi.org/10.1016/J.CHEMOSPHERE.2022.136294