1. “Dispersion in the wake of a rectangular building : validation of two Reynolds-averaged Navier-Stokes modelling approaches”. Gorlé C, van Beeck J, Rambaud P, Boundary-layer meteorology 137, 115 (2010).   http://doi.org/10.1007/s10546-010-9521-0