1. “From streambed temperature measurements to spatial-temporal flux quantification : using the LPML method to study groundwater-surface water interaction”. Anibas C, Schneidewind U, Vandersteen G, Joris I, Seuntjens P, Batelaan O, Hydrological processes 30, 203 (2016).   http://doi.org/10.1002/HYP.10588