1. “New method for selective Cr recovery from stainless steel slag by NaOCl assisted alkaline leaching and consecutive BaCrO4 precipitation”. Kim E, Spooren J, Broos K, Nielsen P, Horckmans L, Vrancken KC, Quaghebeur M, Chemical engineering journal 295, 542 (2016).   http://doi.org/10.1016/J.CEJ.2016.03.073