1. “Optimization of experimental conditions of thin-window EPMA for ligh-element analysis of individual environmental particles”. Szalóki I, Osán J, Worobiec A, de Hoog J, Van Grieken R, X-ray spectrometry 30, 143 (2001).   http://doi.org/10.1002/XRS.473.ABS