1. “Screen versus cyclone for improved capacity and robustness for sidestream and mainstream deammonification”. Van Winckel T, Vlaeminck SE, Al-Omari A, Bachmann B, Sturm B, Wett B, Takács I, Bott C, Murthy SN, De Clippeleir H, Environmental Science: Water Research & Technology 5, 1769 (2019).   http://doi.org/10.1039/C9EW00384C