1. “Selective recovery of Cr from stainless steel slag by alkaline roasting followed by water leaching”. Kim E, Spooren J, Broos K, Horckmans L, Quaghebeur M, Vrancken KC, Hydrometallurgy 158, 139 (2015).   http://doi.org/10.1016/J.HYDROMET.2015.10.024