1. “3D-printed microneedle-based potentiometric sensor for pH monitoring in skin interstitial fluid”. Parrilla M, Vanhooydonck A, Johns M, Watts R, De Wael K, Sensors and actuators : B : chemical 378, 133159 (2023).   http://doi.org/10.1016/J.SNB.2022.133159