1. “Optimizing control strategies for urine nitrification : narrow pH control band enhances process stability and reduces nitrous oxide emissions”. Faust V, Boon N, Ganigué R, Vlaeminck SE, Udert KM, Frontiers in environmental science 11, 1275152 (2023).   http://doi.org/10.3389/FENVS.2023.1275152