1. “Ammonia stripping and scrubbing followed by nitrification and denitrification saves costs for manure treatment based on a calibrated model approach”. Vingerhoets R, Brienza C, Sigurnjak I, Buysse J, Vlaeminck SE, Spiller M, Meers E, Chemical engineering journal 477, 146984 (2023).   http://doi.org/10.1016/J.CEJ.2023.146984