1. “CO₂ electrochemical reduction with Zn-Al layered double hydroxide-loaded gas-diffusion electrode”. Nakazato R, Matsumoto K, Yamaguchi N, Cavallo M, Crocella V, Bonino F, Quintelier M, Hadermann J, Rosero-navarro NC, Miura A, Tadanaga K, Electrochemistry 91, 097003 (2023).   http://doi.org/10.5796/ELECTROCHEMISTRY.23-00080