1. “A hard oxide semiconductor with a direct and narrow bandgap and switchable pn electrical conduction”. Ovsyannikov SV, Karkin AE, Morozova NV, Shchennikov VV, Bykova E, Abakumov AM, Tsirlin AA, Glazyrin KV, Dubrovinsky L, Advanced materials 26, 8185 (2014).   http://doi.org/10.1002/adma.201403304