1. “Modeling SiH4/O2/Ar inductively coupled plasmas used for filling of microtrenches in shallow trench isolation (STI)”. Tinck S, Bogaerts A, Plasma processes and polymers 9, 522 (2012).   http://doi.org/10.1002/ppap.201100093