1. “Reducing the formation of FIB-induced FCC layers on Cu-Zn-Al austenite”. Zelaya E, Schryvers D, Microscopy research and technique 74, 84 (2011).   http://doi.org/10.1002/jemt.20877