1. “Improving the Conversion and Energy Efficiency of Carbon Dioxide Splitting in a Zirconia-Packed Dielectric Barrier Discharge Reactor”. van Laer K, Bogaerts A, Energy technology 3, 1038 (2015).   http://doi.org/10.1002/ente.201500127