1. “Concurrent effects of wafer temperature and oxygen fraction on cryogenic silicon etching with SF6/O2plasmas”. Tinck S, Tillocher T, Georgieva V, Dussart R, Neyts E, Bogaerts A, Plasma processes and polymers 14, 1700018 (2017).   http://doi.org/10.1002/ppap.201700018