1. “Electrorheological fluids with high shear stress based on wrinkly tin titanyl oxalate”. Wu J, Zhang L, Xin X, Zhang Y, Wang H, Sun A, Cheng Y, Chen X, Xu G, ACS applied materials and interfaces 10, 6785 (2018).   http://doi.org/10.1021/ACSAMI.8B00869