1. “Removal of micropollutants from water in a continuous-flow electrical discharge reactor”. Wardenier N, Vanraes P, Nikiforov A, Van Hulle SWH, Leys C, Journal of hazardous materials 362, 238 (2019).   http://doi.org/10.1016/J.JHAZMAT.2018.08.095