1. “Determination of total selenium content in cereals and bakery products by flow injection hydride generation graphite furnace atomic absorption spectrometry applying in-situ trapping on iridium-treated graphite platforms”. Ajtony Z, Szoboszlai N, Bella Z, Bolla S, Szakál P, Bencs L, Microchimica acta 150, 1 (2005).   http://doi.org/10.1007/S00604-005-0330-Y