1. “Electrochemical in situ pH control enables chemical-free full urine nitrification with concomitant nitrate extraction”. De Paepe J, Clauwaert P, Gritti MC, Ganigue R, Sas B, Vlaeminck SE, Rabaey K, Environmental Science & Technology 55, 8287 (2021).   http://doi.org/10.1021/ACS.EST.1C00041