1. “Quasi 3D modelling of vadose zone soil-water flow for optimizing irrigation strategies : challenges, uncertainties and efficiencies”. Rezaei M, De Pue J, Seuntjens P, Joris I, Cornelis W, Environmental modelling and software 93, 59 (2017).   http://doi.org/10.1016/J.ENVSOFT.2017.03.008