1. “Selective leaching of Pb, Cu, Ni and Zn from secondary lead smelting residues”. Kim E, Horckmans L, Spooren J, Vrancken KC, Quaghebeur M, Broos K, Hydrometallurgy 169, 372 (2017).   http://doi.org/10.1016/J.HYDROMET.2017.02.027