1. “Temperature impact on sludge yield, settleability and kinetics of three heterotrophic conversions corroborates the prospect of thermophilic biological nitrogen removal”. Vandekerckhove TGL, De Mulder C, Boon N, Vlaeminck SE, Bioresource technology 269, 104 (2018).   http://doi.org/10.1016/J.BIORTECH.2018.08.012