1. “Total electron yield (TEY) detection mode Cr K-edge XANES spectroscopy as a direct method to probe the composition of the surface of darkened chrome yellow (PbCr1-xSxO4) and potassium chromate paints”. Monico L, d'Acapito F, Cotte M, Janssens K, Romani A, Ricci G, Miliani C, Cartechini L, Nuclear instruments and methods in physics research: B: beam interactions with materials and atoms 539, 141 (2023).   http://doi.org/10.1016/J.NIMB.2023.03.040